# Harmonic Analysis - Running the Computation

In this problem, we are not changing any of the boundary conditions. We are still applying a 1V amplitude signal to the input section, and letting the output in open-circuit conditions. Therefore, we do not need to regenerate the mesh.
Make sure to save your problem (File | Save), and start the computation (Calculate | Calculate).

Previous | TOC | Next