You can verify that all potentials are correctly applied by selecting Draw | Colors.
In this last picture, it is easy to see where the ground, floating, and forced potentials are applied. The other values displayed here have no importance, except for the two immediately following the word "Forced." These values, 1.0 and 0.0, represent the amplitude and phase of the excitation signal.

Previous | TOC | Next