Select the 3 Points XZ definition mode, for instance.
Here, it is convenient to use geometry points to define the center and directions of the local axes. Remember that it is also possible to enter point coordinates in the command line.
To use the mouse cursor to select the points, click once on the lower left corner of the PZT region. GiD should prompt you to use the existing point. Click Join. Repeat for the top left and lower right points to define the local axes.

Previous | TOC | Next