## D. Listing Node Displacements: ATLIST

After running a solver, the user can output thedisplacements for a selected frequency, time or loading case, exactly as theoutput of the solver when the PRINTING level is set to1 or more. He or she can also output the displacement for several specificnodes and degrees of freedom for all frequencies, times or loading cases. Theseactions are driven by the ATLIST program.