## C. User Dialog

System_prompt> ga has04

<<< ATILA Version 5.1.1 >>>
Job name ?
Enter extension name
The width of the CPDDC array is set to 7
Skyline storage without losses.
The number of loading cases is set to 4 .
RADIATING STRUCTURE MODELLING
(SINGLE PRECISION CALCULATION)
(USING MONOPOLAR DAMPERS)
Element QUAD08E # 1 17:12:09
Element QUAD08E # 2 17:12:09
Element QUAD08E # 3 17:12:09
Element QUAD08E # 4 17:12:09
Element QUAD08E # 5 17:12:09
Element QUAD08E # 6 17:12:09
Element QUAD08E # 7 17:12:09
Element QUAD08E # 8 17:12:09
Element QUAD08E # 9 17:12:09
Element QUAD08E # 10 17:12:09
Element QUAD08E # 11 17:12:10
Element QUAD08E # 12 17:12:10
Element QUAD08E # 13 17:12:10
Element QUAD08P # 1 17:12:10
Element QUAD08P # 2 17:12:10
Element QUAD08E # 1 17:12:10
Element QUAD08E # 2 17:12:10
Element QUAD08E # 3 17:12:10
Element LINE06I # 1 17:12:10
Element LINE06I # 2 17:12:10
Element QUAD08F # 1 17:12:10
Element QUAD08F # 2 17:12:10
Element QUAD08F # 3 17:12:10
Element QUAD08F # 4 17:12:10
Element QUAD08F # 5 17:12:10
Element QUAD08F # 6 17:12:10
Element QUAD08F # 7 17:12:10
Element QUAD08F # 8 17:12:10
Element QUAD08F # 9 17:12:10
Element QUAD08F # 10 17:12:10
Element QUAD08F # 11 17:12:10
Element QUAD08F # 12 17:12:10
Element QUAD08F # 13 17:12:10
Element QUAD08F # 14 17:12:10
Element QUAD08F # 15 17:12:10
Element QUAD08F # 16 17:12:10
Element QUAD08F # 17 17:12:10
Element QUAD08F # 18 17:12:10
Element QUAD08F # 19 17:12:10
Element QUAD08F # 20 17:12:10
Element QUAD08F # 21 17:12:10
Element QUAD08F # 22 17:12:10
Element QUAD08F # 23 17:12:10
Element QUAD08F # 24 17:12:10
Element QUAD08F # 25 17:12:10
Element QUAD08F # 26 17:12:10
Element QUAD08F # 27 17:12:10
Element QUAD08F # 28 17:12:10
Element QUAD08F # 29 17:12:10
Element QUAD08F # 30 17:12:10
Element QUAD08F # 31 17:12:11
Element QUAD08F # 32 17:12:11
Element QUAD08F # 33 17:12:11
Element QUAD08F # 34 17:12:11
Element QUAD08F # 35 17:12:11
Element QUAD08F # 36 17:12:11
Element QUAD08F # 37 17:12:11
Element QUAD08F # 38 17:12:11
Element QUAD08F # 39 17:12:11
Element QUAD08F # 40 17:12:11
Element LINE03R # 1 17:12:11
Element LINE03R # 2 17:12:11
Element LINE03R # 3 17:12:11
Element LINE03R # 4 17:12:11
Element LINE03R # 5 17:12:11
Element LINE03R # 6 17:12:11
Element LINE03R # 7 17:12:11
Block 1 assembling ended.
COMPLEX SIMPLE PRECISION FREQUENCY COMPUTATION.
Frequency 25000.0 Hz -17:12:11
Frequency 26000.0 Hz -17:12:11
Frequency 27000.0 Hz -17:12:11
Frequency 28000.0 Hz -17:12:11
The sound speed used is SSPD= 1489.97
Deduced acoustic center : ( 0.00000 , 0.00000 ) ,
Structure symmetric relative to the X axis.
Structure symmetric relative to the Y axis.
NC = 12
Frequency = 25000.0 Hz, number of directivity terms = 7
Frequency = 26000.0 Hz, number of directivity terms = 7
Frequency = 27000.0 Hz, number of directivity terms = 7
Frequency = 28000.0 Hz, number of directivity terms = 7
DATE:10/20/97 AT:17:12:12 END OF JOB:HAS04 CPU TIME: 7.91 SEC.