# Generating the Mesh

ATILA requires that the mesh be composed exclusively of second order elements. The corresponding setting can be found under the Meshing menu. Select Quadratic Elements, then Quadratic. Note that this option is automatically set when you start the ATILA-GiD interface.
For the transformer, we will define a structured mesh. Select Structured | Volumes from the Meshing menu.

Previous | TOC | Next